*Dimensions in mm*

**Front A-Arms**

|  |  |  |
| --- | --- | --- |
|  | X | Y |
| **Top** | | |
| Front | 245 | 307.02 |
| Rear | 245 | 292.72 |
| Spherical Holder | 502.56 | 298.98 |
| **Bottom** | | |
| Front | 105.94 | 145.76 |
| Rear | 105.94 | 145.76 |
| Spherical Holder | 531.71 | 104.46 |
| Bottomaarmtobottomchassis | 72.03 |  |

**Rear A-Arms**

|  |  |  |
| --- | --- | --- |
|  | X | Y |
| **Top** | | |
| Front | 308.17 | 276.99 |
| Rear | 289.17 | 283.43 |
| Spherical Holder | 490.41 | 298.77 |
| **Bottom** | | |
| Front | 287.61 | 120.78 |
| Rear | 268.8 | 122.03 |
| Spherical Holder | 531.71 | 104.46 |
| Bottomaarmtobottomchassis | 50.52 |  |

**Differences & Angles**  
Tyre Diameter: 406.4  
Tyre Radius: 203.2

Front KPI: 7.5 degrees  
Rear KPI: 11 degrees